|  |  |  |
| --- | --- | --- |
|  |  | SESIP Profile for PSA Certified™ Level 2 |



|  |  |
| --- | --- |
| Document number:  | JSADEN012 |
| Version: | 2.0 REL |
| Release Number: | 01 |
| Author | PSA JSA Members:Applus+ LaboratoriesArm LimitedCAICTDEKRA Testing and CertificationECSEC Laboratory IncProvenRun S.A.S.Riscure B.V.Serma Safety & Security S.A.S.SGS Brightsight B.V.TrustCB B.V.UL TS B.V. |
| Authorized by: | PSA JSA Members |
| Date of Issue: | 28/03/2024 |

© Copyright Arm Limited 2017-2024. All rights reserved.

Abstract

PSA Certified is the independent security evaluation scheme for Platform Security Architecture (PSA) based IoT systems. It establishes trust through a multi-level assurance program for chips containing a security component called a Root of Trust (PSA-RoT) that provides trusted functionality to the platform. The multi-level scheme has been designed to help device makers and businesses get the level of security they need for their use case. An overview of SESIP Profiles important to the PSA Certified scheme is given in Figure 1 that shows how this document relates to others for the chip’s Root of Trust.

PSA Certified Level 2 is a fixed time, test laboratory based, evaluation of the PSA-RoT. It is aimed at IoT devices that need to protect against basic software attacks. The Level 2 documents include: a SESIP Profile that describes the Target of Evaluation, its assets, the security objectives and security functions that will be evaluated and an Attack Methods (AM) document describing the attacks in scope.

Developers submit their PSA-RoT to an approved test laboratory, listed on [www.psacertified.org](http://www.psacertified.org), for Level 2 evaluation and receive an Evaluation Technical Report. If the PSA-RoT is assessed as passing and approved by the independent Certification Body, a digital certificate will be issued on the PSA Certified website.

Keywords

PSA Certified Level 2, SESIP, Certification, IoT, Platform Security Architecture, Questionnaire, PSA, Security



Figure 1: PSA Certified SESIP Profiles for the chip’s RoT

Copyright ©2017-2024 Arm Limited or its affiliates. All rights reserved. The copyright statement reflects the fact that some draft issues of this document have been released, to a limited circulation.

## Non-Confidential Proprietary Notice

This document is protected by copyright and other related rights and the practice or implementation of the information contained in this document may be protected by one or more patents or pending patent applications. No part of this document may be reproduced in any form by any means without the express prior written permission of Arm. No license, express or implied, by estoppel or otherwise to any intellectual property rights is granted by this document unless specifically stated.

Your access to the information in this document is conditional upon your acceptance that you will not use or permit others to use the information for the purposes of determining whether implementations infringe any third-party patents.

THIS DOCUMENT IS PROVIDED “AS IS”. ARM PROVIDES NO REPRESENTATIONS AND NO WARRANTIES, EXPRESS, IMPLIED OR STATUTORY, INCLUDING, WITHOUT LIMITATION, THE IMPLIED WARRANTIES OF MERCHANTABILITY, SATISFACTORY QUALITY, NON-INFRINGEMENT OR FITNESS FOR A PARTICULAR PURPOSE WITH RESPECT TO THE DOCUMENT. For the avoidance of doubt, Arm makes no representation with respect to, and has undertaken no analysis to identify or understand the scope and content of, patents, copyrights, trade secrets, or other rights.

This document may include technical inaccuracies or typographical errors.

TO THE EXTENT NOT PROHIBITED BY LAW, IN NO EVENT WILL ARM BE LIABLE FOR ANY DAMAGES, INCLUDING WITHOUT LIMITATION ANY DIRECT, INDIRECT, SPECIAL, INCIDENTAL, PUNITIVE, OR CONSEQUENTIAL DAMAGES, HOWEVER CAUSED AND REGARDLESS OF THE THEORY OF LIABILITY, ARISING OUT OF ANY USE OF THIS DOCUMENT, EVEN IF ARM HAS BEEN ADVISED OF THE POSSIBILITY OF SUCH DAMAGES.

This document consists solely of commercial items. You shall be responsible for ensuring that any use, duplication or disclosure of this document complies fully with any relevant export laws and regulations to assure that this document or any portion thereof is not exported, directly or indirectly, in violation of such export laws. Use of the word “partner” in reference to Arm’s customers is not intended to create or refer to any partnership relationship with any other company. Arm may make changes to this document at any time and without notice.

If any of the provisions contained in these terms conflict with any of the provisions of any click through or signed written agreement covering this document with Arm, then the click through or signed written agreement prevails over and supersedes the conflicting provisions of these terms. This document may be translated into other languages for convenience, and you agree that if there is any conflict between the English version of this document and any translation, the terms of the English version of the Agreement shall prevail.

The Arm corporate logo and words marked with ® or ™ are registered trademarks or trademarks of Arm Limited (or its subsidiaries) in the US and/or elsewhere. All rights reserved.  Other brands and names mentioned in this document may be the trademarks of their respective owners. Please follow Arm’s trademark usage guidelines at <http://www.arm.com/company/policies/trademarks>.

Copyright © 2024 Arm Limited (or its affiliates). All rights reserved.

Arm Limited. Company 02557590 registered in England.

110 Fulbourn Road, Cambridge, England CB1 9NJ.

Contents

Non-Confidential Proprietary Notice 3

1 About this document 6

1.1 Current Status and Anticipated Changes 6

1.2 Release Information 6

1.3 References 7

1.3.1 Normative references 7

1.3.2 Informative references 7

1.4 Terms and Abbreviations 8

1.5 PSA Certified Level 2 10

1.5.1 PSA Certified Level 2 Ready Evaluation 10

1.5.2 PSA Certified Level 2+SE Certification 10

1.5.3 PSA Certified RoT Component Certification 10

2 Introduction 12

2.1 SESIP Profile Reference 12

2.2 Platform Reference 12

2.3 Included Guidance Documents 13

2.4 Platform Functional Overview and Description 13

2.4.1 Platform Type 13

2.4.2 Physical Scope 14

2.4.3 Logical Scope 15

2.4.4 Usage and Major Security Features 16

2.4.5 Required Hardware/Software/Firmware 16

3 Security Objectives for the operational environment 17

4 Security Requirements and Implementation 18

4.1 Security Assurance Requirements 18

4.1.1 Flaw Reporting Procedure (ALC\_FLR.2) 18

4.2 Base PP Security Functional Requirements 18

4.2.1 Verification of Platform Identity 18

4.2.2 Verification of Platform Instance Identity 18

4.2.3 Attestation of Platform Genuineness 18

4.2.4 Secure Initialization of Platform 19

4.2.5 Attestation of Platform State 19

4.2.6 Secure Update of Platform 19

4.2.7 Software Attacker Resistance: Isolation of Platform (between SPE and NSPE) 19

4.2.8 Software Attacker Resistance: Isolation of Platform (between PSA-RoT and Application Root of Trust Services) 20

4.2.9 Cryptographic Operation 20

4.2.10 Cryptographic Random Number Generation 20

4.2.11 Cryptographic Key Generation 21

4.2.12 Cryptographic KeyStore 21

4.3 Optional Security Functional Requirements 21

4.3.1 Audit Log Generation and Storage 21

4.3.2 Software Attacker Resistance: Isolation of Application Parts (between each of the Application Root of Trust services) 22

4.3.3 Secure Debugging 22

4.3.4 Secure Encrypted Storage 22

4.3.5 Secure Confidential Storage 22

4.3.6 Secure Trusted Storage 23

4.3.7 Secure Data Serialization 23

4.3.8 Limited Physical Attacker Resistance 23

4.3.9 Secure Communication Support 24

4.3.10 Secure Communication Enforcement 24

5 Mapping and Sufficiency Rationales 25

5.1 Assurance 25

6 Appendix: SFRs by PSA Certified Levels 27

# About this document

## Current Status and Anticipated Changes

Current Status: Released, version 2.0 REL 01

## Release Information

The change history table lists the changes that have been made to this document.

|  |  |  |  |
| --- | --- | --- | --- |
| Date | Version | Confidentiality | Change |
| 2020-12-09 | 1.0ALP01 | Non-confidential | Initial version to be discussed with JSA members  |
| 2021-01-27 | 1.0BET01 | Non-confidential | Updates discussed with JSA members  |
| 2020-02-10 | 1.0BET02 | Non-confidential | Feedback provided by JSA members |
| 2020-04-11 | 1.0BET04 | Non-confidential | External partner review |
| 2022-10-10 | 1.0 REL 01 | Non-confidential | Clearer support for Trusted Sub-systems and L2+SE |
| 2022-11-24 | 1.0 REL 02 | Non-confidential | + Abstract |
| 2023-08-07 | 1.0 REL 03 | Non-confidential | Update to include Secure Confidential Storage from prEN17927 as non SESIP SFR |
| 2023-10-12 | 1.0 REL 04 | Non-confidential | Alignment with SESIP 1.2 and minor updates |
| 2024-02-02 | 2.0 REL 01 | Non-confidential | Minor edits for publication |

## References

This document refers to the following documents.

### Normative references

|  |  |  |  |
| --- | --- | --- | --- |
| Ref | Doc No | Author(s) | Title |
| [PSA-L1] | JSADEN001 | JSA | PSA Certified Level 1 Questionnaire |
| [PSA-EM-L2] | JSADEN003 | JSA | PSA Certified: Evaluation Methodology for PSA L2 |
| [PSA-EM-L3] | JSADEN010 | JSA | PSA Certified: Evaluation Methodology for PSA L3 |
| [PSA-AM] | JSADEN004 | JSA | PSA Certified Attack Methods |
| [PSA-PP-L2] | JSADEN002 | JSA | PSA Certified Level 2 Lightweight Protection Profile |
| [PSA-PP-L3] | JSADEN009 | JSA | PSA Certified Level 3 Lightweight Protection Profile |
| [SESIP-PP-L3] | JSADEN011 | JSA | SESIP Profile for PSA Certified™ Level 3 |
| [PSA-L2-COMP] | JSADEN017 | JSA | SESIP Profile for PSA Certified™ RoT Component Level 2 |
| [PSA-L3-COMP] | JSADEN018 | JSA | SESIP Profile for PSA Certified™ RoT Component Level 3 |
| [PSA-L4-iSE-SE] | JSADEN023 | JSA | SESIP Profile for PSA Certified™ Level 4 iSE/SE and RoT Component |
| [SESIP] | GP\_FST\_070 | GlobalPlatform | Security Evaluation Standard for IoT Platforms (SESIP) v1.2 |
| [CEN-SESIP] | EN 17927 | CEN/CENELEC | Security Evaluation Standard for IoT Platforms (SESIP) 2023 |
| [CEM] | CCMB-2017-04-004 | Common Criteria | Common Methodology for Information Technology Security Evaluation, Evaluation Methodology. Version 3.1, revision 5, April 2017.  |

### Informative references

| Ref | Doc No | Author(s) | Title |
| --- | --- | --- | --- |
| [GP-ROT] | GP\_REQ\_025 | GlobalPlatform | Root of Trust Definitions and Requirements, Version 1.1, Public Release, June 2018 |
| [PSA-SM] | JSADEN014 | ARM | Platform Security Model |
| [PSA-SS] | IHI 0087 | ARM | PSA Certified Secure Storage API, Version 1.0 or later |
| [SP-800-57] | SP 800-57 Part 1  | NIST | Recommendation for Key Management: Part 1 – General, Rev. 5 |

## Terms and Abbreviations

This document uses the following terms and abbreviations (see PSA-SM and PSA-L1).

| Term | Meaning |
| --- | --- |
| Application | Used in this SESIP profile to refer to the components which are out of the scope of the evaluation. |
| Application Root of Trust Service(s) | Application specific security service(s) that are not defined by PSA. Such services execute in the Secure Processing Environment and are required to be in Secure Partitions. |
| Application Specific Software | Software that provides the functionality required of the specific device. This software runs in the Non-Secure Processing Environment, making use of the System Software, Application RoT Services and PSA-RoT Services.  |
| Critical Security Parameter | Secret information, with integrity and confidentiality requirements, used to maintain device security, such as authentication data (passwords, PIN, certificates), secret cryptographic keys, etc.. |
| Evaluation Laboratory | Laboratory or facility that performs the assessment of products submitted for PSA Certified. The list of evaluation laboratories participating to PSA Certified can be found on www.psacertified.org |
| Hardware Unique Key (HUK) | Secret and unique to the device symmetric key that must not be accessible outside the PSA Root of Trust. It is a Critical Security Parameter. |
| Host Platform  | The entity which when used in composition with a certified PSA Level 2 RoT Component [PSA-L2-COMP], a certified PSA Level 3 RoT Component [PSA-L3-COMP] or a certified PSA Level 4 RoT Component [PSA-L4-iSE-SE] form the scope of the certification covered in this profile. |
| Initial Attestation Key (IAK)  | A PSA-RoT secret private key from an asymmetric key-pair used to sign attestation reports, thus ensuring that the report is bound to a unique PSA- RoT (and so device) instance. |
| Non-secure Processing Environment (NSPE) | The processing environment that hosts the non-secure System Software and Application Specific Software. PSA requires the NSPE to be isolated from the SPE. Isolation between partitions within the NSPE is not required by PSA though is encouraged where supported. |
| Partition | The logical boundary of a software entity with intended interaction only via defined interfaces, but not necessarily isolated from software in other partitions. Note that both the NSPE and SPE may host partitions.  |
| Platform | Used in this SESIP Profile to refer to the components which are in the scope of the evaluation. |
| PSA | Platform Security Architecture |
| PSA Certification Body | The entity that receives applications for PSA security certification, issues the certificates, maintains the security certification scheme, and ensures consistency across all the evaluation laboratories. |
| PSA Functional APIs | PSA defined Application Programming Interfaces on which security services can be built. APIs defined so far include Crypto, Secure Storage and Attestation. |
| PSA Functional API Certification | Functional certification confirms that the device implements the PSA Functional APIs correctly by passing the PSA Functional certification test suites. |
| PSA Root of Trust (PSA-RoT) | The PSA defined combination of the Immutable Platform Root of Trust and the Updateable Platform Root of Trust and is considered to be the most trusted security component on the device. See [PSA-SM]. |
| Immutable Platform Root of Trust | The minimal set of hardware, firmware and data of the PSA-RoT, which is inherently trusted because it cannot be modified following manufacture. There is no software at a deeper level that can verify that it as authentic and unmodified.  |
| Updateable Platform Root of Trust | The firmware, software and data of the PSA-RoT that can be securely updated following manufacture. |
| Platform Root of Trust Service(s) | PSA defined security services for use by PSA-RoT, Application RoT Service(s) and by the NSPE. Executes in the Secure Processing Environment and may use Trusted Subsystems. This includes the services offered by the PSA Functional APIs. |
| SESIP Profile | Document providing a common set of functionalities for similar products |
| Secure Partition | A Partition in the Secure Processing Environment. |
| Secure Processing Environment Partition Management | Management of the execution of software in Secure Partitions. Typical implementations will provide scheduling and inter partition communication mechanisms. Implementations may also enforce isolation between the managed Secure Partitions. |
| Secure Processing Environment (SPE) | The processing environment that hosts the PSA-RoT, the PSA-RoT Services, and any Application RoT Service(s). |
| Secure Boot | The process of verifying and validating the integrity and authenticity of updateable firmware and software components as a pre-requisite to their execution. This must apply to all the firmware and software in the SPE. It should also apply to the first NSPE image loaded, which may extend the NSPE secure boot chain further. |
| Security Target (ST) | Document providing an implementation-dependent statement of security of a specific identified platform. |
| System Software | NSPE software that may comprise an Operating System or some run-time executive, together with any middleware, standard stacks and libraries, chip specific device drivers, etc., but not the application specific software. |
| TOE | Target of Evaluation. In this SESIP Profile it is a synonym for Platform. |
| Trusted subsystem | A security subsystem that the PSA-RoT relies on for protection of its assets, or that implement some of its services.  |

## PSA Certified Level 2

PSA defines a common hardware and software security platform, providing a generic security foundation and allowing secure products and features to be developed on top of this platform.

The PSA Certified scheme involves the evaluation by a laboratory of a device against a set of security requirements and, in case of a successful evaluation, the certification by the PSA Certified certification body of this Platform. The evaluation laboratory examines measures and processes to ensure that a functional Platform is not vulnerable to the identified threats to the levels defined in this document.

The PSA programme recognises that there will be different security requirements and different cost/security trade-offs for different applications and eco-systems. This is reflected in specifications by introducing a range of assurance levels.

Two evaluation paths are currently possible for a PSA Certified Level 2 product, either through the PSA Certified Level 2 Protection Profile [PSA-PP-L2] and associated evaluation methodology [PSA-EM-L2], or through a SESIP evaluation using the SESIP Profile defined in this document. The SESIP standard associated with this document is defined either by GlobalPlatform [GP-SESIP] or by CEN/CENELEC [CEN-SESIP].

### PSA Certified Level 2 Ready Evaluation

The PSA Certified scheme allows for pre-certification evaluation of FPGA or development-based systems, which provide reference designs for ASIC or custom chip, but which may not be able to meet all security functions of this profile. In this case, only the claimed security functions are tested by the Evaluation Laboratory who issues the Evaluation Technical Report. No PSA Certified Level 2 certificate is generated for a Level 2 Ready evaluation, but the Developer can obtain the rights to use a specific “PSA Certified Level 2 Ready” logo and showcase its solution on [www.psacertified.org](http://www.psacertified.org).

Such a logo could be used to demonstrate, for example, the benefit of software security assurance offered from an evaluated FPGA based system for development of secure AROTs, RTOS or device while maximizing chances of passing PSA Certified Level 2 certification for future ASIC or custom chips based on the FPGA reference design.

### PSA Certified Level 2+SE Certification

The PSA Certified scheme also considers a PSA Certified Level 2 certification where the product architecture, as illustrated in Figure 2, includes a trusted subsystem, typically an external Secure Element or an on-chip integrated Secure Element.

The Developer can obtain the rights to use the specific “PSA Certified Level 2+SE” logo and showcase the solution on [www.psacertified.org](http://www.psacertified.org), when the trusted subsystem has been certified for the security functions listed below for protection against physical attacks to at least PSA Certified Level 3 RoT Component [PSA-L3-COMP], or SESIP3, or AVA\_VAN.3 (with Common Criteria).

The L2+SE logo could be used to demonstrate, for example, the benefit of protection against hardware attacks for the most sensitive assets of the product.

### PSA Certified RoT Component Certification

The PSA Certified scheme allows for certification of RoT Components that address a subset of the security functions required by an implementation for a Level 2 certifiable PSA Root-of-Trust (RoT) in accordance with this protection profile.

In the PSA Security Model [PSA-SM] such parts of a root-of-trust are referred to as a Trusted Subsystem. A typical example is an IP block that will be used in a chip. The IP could address a few security functions, with the rest of the chip covering all other requirements. Another example is an external chip that addresses a subset of the security functions, which when connected to another chip (Host Platform) form a complete Level 2 certifiable PSA-Root-of-Trust.

A PSA L2 RoT Component [PSA-L2-COMP] may be used to aid the evaluation of an L2 PSA-RoT certification.

# Introduction

This SESIP profile proposes a mapping between the security functionality defined in the PSA L2 Protection Profile [PSA-PP-L2] and the SFRs (Security Functional Requirements) listed in the SESIP catalogue [SESIP]. This profile also includes some optional SFRs aiming to cover most of the platform use cases.

The effort for performing the AVA\_VAN.2 activities of a standard implementation of a PSA-RoT is **25 person-days**. It is assumed for this workload that:

* the source code for the components in scope of the platform (see Sections 2.4.2 and 2.4.3, hardware design is not required). This shall include drivers for Trusted Subsystems if used;
* no additional SFRs are added in the Profile;
* evaluation activities are not re-used;
* the SFRs “Cryptographic Operation” and “Cryptographic Key Generation” include one cryptographic algorithm;
* the platform does not rely on a certified trusted subsystem or certified PSA Certified RoT Component (see Sections 1.5.2 and 1.5.3).

|  |
| --- |
| Reading guide:In the document there is guidance information aiming to facilitate reader understanding. This information can be easily identified as it is included in tables with a grey background:REQ: guidance that shall be considered and followed for the Security Target writing.INFO: clarification to be considered. |

## SESIP Profile Reference

|  |  |
| --- | --- |
| Reference | Value |
| PP Name | SESIP Profile for PSA Certified Level 2 |
| PP Version | See title page. |
| Assurance Claim | SESIP Assurance Level 2 (SESIP2) |
| SESIP Standard | *<[GP-SESIP] or [CEN-SESIP]>* |
| Optional and additional SFRs | <TBD> |

Table 1: SESIP Profile Reference

## Platform Reference

The platform is uniquely identified by its chip (hardware) reference and its PSA defined Root of Trust (software) reference as described below. The developer declares that only the evaluated and successfully certified products identify in this way.

|  |  |
| --- | --- |
| Reference | Value |
| Platform Name | <TBD> |
| Platform Version | <TBD> |
| Platform Identification | Chip name and version |  |
| PSA-RoT name and version |  |
| Platform Type | <TBD> |
| Trusted Subsystem Identification | <If a trusted subsystem is used, provide reference such as chip name, part number and version.> |
| Trusted Sub-system Certification | <If a certified trusted subsystem is used please provide the PSA Certificate EAN-13 reference or another identifier.> |

Table 2: Platform Reference

## Included Guidance Documents

The following documents are included with the platform:

|  |  |  |
| --- | --- | --- |
| Reference | Name | Version |
| <[Ref1]> | <Full title of the document> | <Vx.y> |
|  |  |  |

Table 3: Guidance Documents

|  |  |
| --- | --- |
| REQ | The guidance shall list all the documents that will be provided to the evaluator for the documentation review, covering AGD\_OPE.1 and AGD\_PRE.1. This documentation is expected to be available to the customers without restrictions. |

## Platform Functional Overview and Description

### Platform Type

<The developer must choose an appropriate Platform type.> Some examples are:

* Processor with internal hardware isolation, such as Arm TrustZone technology, and secure memory.
* Processor with multiple cores where one is dedicated to security.
* Processor with external trusted subsystem, such as a Secure Element or secure storage device.
* Use of a separate security processor with secure memory.

Note that secure memory may be integral to the die, on a separate die within the same package or on an external package cryptographically bound to the main chip.

|  |  |
| --- | --- |
| REQ | As stated before, these are examples of different Platform types. The developer shall fill this section based on the evaluated product. |
| REQ | When a trusted subsystem is relied upon for operation of the PSA Root of Trust, such as an on-chip security subsystem or off-chip Secure Element, the developer shall describe usage of the trusted subsystem, such as, cryptographic provider for the Platform Root-of-Trust and Application Root-of-Trust.The developer may reference any existing security certification of the Trusted Subsystem, such as PSA Certified RoT Component, SESIP, FIPS-140, or Common Criteria. If any existing security certification is not sufficient to cover the trusted subsystem security functions relied upon to establish the PSA Root of Trust, the developer can pre-certify these security functions by:* a PSA Certified Level 2 RoT Component certification [PSA-L2-COMP] or
* a PSA Certified Level 3 RoT Component certification [PSA-L3-COMP] or
* a PSA Certified Level 4 RoT Component certification [PSA-L4-iSE-SE]

Otherwise, these security functions will be evaluated within the scope of the PSA Certified Level 3 security evaluation. |

### Physical Scope

The hardware is a <System-on-Chip or a System-in-Package or a discrete solution all with board level integration>.

The hardware is in the scope of the security evaluation as it provides security features, such as immutable storage or protection of JTAG, which are essential for ensuring the security of the implementation.

<write specific scope details, which may be a silicon chip, a PCB, …>

### Logical Scope

The scope for a SESIP Security evaluation, or Target of Evaluation (TOE), according to this profile is the combination of the trusted hardware and firmware components implementing a PSA-RoT with the Security Functional Requirements stated in this document, see Figure 2.



Figure 2: Scope of PSA Certified Level 2

The Chip security evaluation scope includes the following Secure Processing Environment PSA-RoT elements, as described in [PSA-SM]:

* Immutable Platform Root of Trust, for example, the Boot ROM, any root parameters, the NSPE/SPE isolation hardware, and any hardware-based security lifecycle management and enforcement.
* Updateable Platform Root of Trust, for example, a main bootloader, the code that implements the SPE Partition Management function, the code that implements the PSA defined services such as attestation, secure storage, and cryptography.
* Any Trusted subsystems that the host processor relies on for protection of its assets, or that implement some of its services.

The Platform scope hardware may be a System-on-Chip or a System-in-Package, possibly supported by board level trusted subsystem components, for example, a Secure Element or Subscriber Identification Module.

<complete this section with the logical scope of the evaluated product>

### Usage and Major Security Features

This profile considers the following features for the purpose of PSA Level 2 security evaluation:

* A Secure Processing Environment (SPE) isolated by hardware mechanisms to protect critical services and related assets from the Non-Secure Processing Environment.
* A Secure Boot process to verify integrity and authenticity of executable code in a chain of trust starting from the Boot ROM. Related certificates are protected in integrity by hardware mechanisms.
* Support for Secure Storage, to protect in integrity and confidentiality sensitive assets for the SPE and related applications. These assets include at least the Hardware Unique Key (HUK), the PSA-RoT Public Key (ROTPK), the Initial Attestation Key (IAK), and the unique instance ID.
* A Security Lifecycle for the SPE, to protect the lifecycle state for the device and enforce the transition rules between states.
* Cryptographic functions services for SPE and SPE applications.
* Support for an attestation method, for example Entity Attestation Token (according to IETF specification).

<complete this section with the additional information from the evaluated product>

### Required Hardware/Software/Firmware

<clarify if the Platform is supplied with existing apps, Application Root of Trust Services or other components>

# Security Objectives for the operational environment

For the platform to fulfil its security requirements, the operational environment (technical or procedural) must fulfil the following objectives.

|  |  |  |
| --- | --- | --- |
| ID | Description | Reference |
| KEY\_MANAGEMENT | Cryptographic keys and certificates outside of the platform are subject to secure key management procedures. | *<[Ref1]>* Section X |
| TRUSTED\_USERS | Actors in charge of platform management, for instance for signature of firmware update, are trusted. | *<[Ref1]>* Section X |
| UNIQUE\_ID | The integrity and uniqueness of the unique identification of the platform must be provided by the platform user during the personalization stage. | *<[Ref1]>* Section X |
| <TBD> | <TBD> | <TBD> |

Table 4: Security Objectives for the Operational Environment

|  |  |
| --- | --- |
| INFO | Additional Objectives for the Environment may be added. |
| REQ | The guidance shall list all the documents that will be provided to the evaluator for the documentation review, covering AGD\_OPE.1 and AGD\_PRE.1. This documentation shall be available to the customers. |
| REQ | The integrity and uniqueness of the unique identification of the Platform should be supported by the development, production, and test environment.Otherwise, if the integrity and uniqueness of the unique identification is responsibility of the Platform user, then the objective for the environment UNIQUE\_ID shall be defined. |

# Security Requirements and Implementation

## Security Assurance Requirements

The SESIP claimed assurance requirements package is **SESIP2** as described in Section 5.1.

### Flaw Reporting Procedure (ALC\_FLR.2)

In accordance with the requirement for a flaw reporting procedure (ALC\_FLR.2), including a process to report flaw and generate any needed update and distribute it, the developer has defined the following procedure:

<Describe the procedure, including where flaws can be reported (website and/or email address), how the reported flaws are handled in a timely manner, and how an application developer/end-user is informed of the update.>

## Base PP Security Functional Requirements

As a base, the platform fulfils the following security functional requirements:

|  |  |
| --- | --- |
| REQ | The “Verification of Platform Identity” and the “Secure Update of Platform” requirements are explicitly listed here, because they are mandatory in all SESIP Security Targets.  |
| REQ | For every SFR, a description of the implementation in the Platform needs to be included. |
| INFO | Statement of the SFRs uses **bold text** to identify places where fields with angle brackets (<>) in the SESIP catalog have been filled with specificities of the platform considered in this Profile. |

### Verification of Platform Identity

The platform provides a unique identification of the platform, including all its parts and their versions.

|  |  |
| --- | --- |
| INFO | This requirement is mandatory according to [SESIP]. |
| REQ | When a trusted subsystem is used for this function, the Chip Vendor shall describe how the trusted subsystem is identified. |

### Verification of Platform Instance Identity

The platform provides a unique identification of that specific instantiation of the platform, including all its parts.

### Attestation of Platform Genuineness

The platform provides an attestation of the “Verification of Platform Identity” and “Verification of Platform Instance Identity”, in a way that ensures that the platform cannot be cloned or changed without detection.

|  |  |
| --- | --- |
| REQ | When a trusted subsystem is used for this function, the Chip Vendor shall describe how attestation is performed and which information is exchanged with the trusted subsystem. |

### Secure Initialization of Platform

The platform ensures its integrity and authenticity during platform initialization. If the platform integrity or authenticity cannot be ensured, the platform will go to **a state where no other operation except optionally Secure Update of Platform can be performed**.

|  |  |
| --- | --- |
| REQ | Secure initialization functionality shall ensure the integrity and authenticity of the:* Updateable PSA Root of Trust and PSA Root of Trust Services
* Trusted Sub-system(s) (if any)
* Application Root of Trust (if any).
 |
| *INFO* | The Secure Initialization should be extendable from the SPE to at least the first image of the NSPE code (see section 1.4). |
| REQ | If the initialization fails, restarts or at most recovery using the update mechanism may be performed. All other functions shall not be available. The application may be used to facilitate this update but shall not provide any other functionality until the authenticity and integrity of the platform is re-established. Any guidance for the application on this shall be explicitly mentioned as a Security Objectives for the operational environment, with explicit reference to where this guidance is provided. |
| REQ | The user guidance shall describe the secure anti-rollback policies that are enforced by the PSA-RoT. A device shall only execute software versions that do not violate the anti-rollback policies. |

### Attestation of Platform State

The platform provides an attestation of the state of the platform, such that it can be determined that the platform is in a known state.

### Secure Update of Platform

The platform can be updated to a newer version in the field such that the **confidentiality,** integrity and authenticity of the platform is maintained.

|  |  |
| --- | --- |
| INFO | PSA-RoT consists of an Immutable Platform RoT and an Updateable Platform RoT. This SFR is only applicable to the updatable parts. |
| REQ | The user guidance shall describe the secure anti-rollback policies that are enforced by the PSA-RoT. A device shall only install software updates of newer versions than the current version on the device. |
| REQ | If parts of the Platform, for example a Host Platform and a Trusted Subsystem can be updated independently, then this SFR shall be iterated to describe each process. |
| INFO | Where an existing valid version remains intact after any update is installed, then the update can be verified and authenticity checked, and downgrade attempts rejected, by the TOE during Secure Initialization. |
| REQ | Where the only existing valid version is lost during any update installation, then the update shall be verified and authenticity checked, and downgrade attempts rejected, by the TOE immediately prior to installation. |

### Software Attacker Resistance: Isolation of Platform (between SPE and NSPE)

The platform provides isolation between the application and itself, such that an attacker able to run code as an application on the platform cannot compromise the other functional requirements.

|  |  |
| --- | --- |
| *INFO* | This requirement must be interpreted as an isolation between SPE and NSPE. |

### Software Attacker Resistance: Isolation of Platform (between PSA-RoT and Application Root of Trust Services)

The platform provides isolation between the application and itself, such that an attacker able to run code as an application on the platform cannot compromise the other functional requirements.

|  |  |
| --- | --- |
| INFO | This requirement must be interpreted as an isolation between the PSA Root of Trust and the Application Root of Trust Services. |

### Cryptographic Operation

The platform provides **Operations in Table 5** functionality with **algorithms in Table 5** as specified in **specifications in Table 5** for key lengths **described** **in Table 5** and modes **described in Table 5**.

| Algorithm | Operations | Specification | Key lengths | Modes |
| --- | --- | --- | --- | --- |
| <TBD> | <TBD> | <TBD> | <TBD> | <TBD> |
| <TBD> | <TBD> | <TBD> | <TBD> | <TBD> |
| <TBD> | <TBD> | <TBD> | <TBD> | <TBD> |

Table 5: Cryptographic Operations

|  |  |
| --- | --- |
| REQ | This SFR addresses the algorithms available to the NSPE. As this SFR is mandatory, at least one cryptographic algorithm shall be included in the scope. |
| REQ | The platform implements some internal functionality that performs cryptographic operations: secure storage, attestation, and boot decryption. The cryptography used by these functions shall be also described in this SFR. |
| *REQ*  | PSA requires minimum security strength in line with the current version of NIST [SP-800-57] recommendations. |
| *INFO*  | RSA 2048 will not be accepted in products certified from 2027 onwards. |
| REQ | When a trusted subsystem is used for some or all of this function, the Chip Vendor shall describe which set of cryptographic operations is performed by the trusted subsystem. |

### Cryptographic Random Number Generation

The platform provides a way based on <list of entropy sources> to generate random numbers to as specified in <specification>.

|  |  |
| --- | --- |
| INFO | This SFR addresses the RNG functionality available to the NSPE. |
| REQ | When a trusted subsystem is used for some, or all, of this function, the Chip Vendor shall describe which part of the random number generation is performed by the trusted subsystem. |
| REQ | If the platform contains multiple random number generators, this SFR shall be iterated to describe each instance. |

### Cryptographic Key Generation

The platform provides a way to generate cryptographic keys for use in **cryptographic algorithms in Table 6** as specified in **specifications in Table 6** for key lengths **described** **in Table 6**.

| ID | Algorithm | Specification­­ | Key lengths |
| --- | --- | --- | --- |
| <TBD> | <TBD> | <TBD> | <TBD> |
| <TBD> | <TBD> | <TBD> | <TBD> |
| <TBD> | <TBD> | <TBD> | <TBD> |

Table 6: Cryptographic Key Generation

|  |  |
| --- | --- |
| REQ | This SFR addresses the key generation algorithms available to the NSPE. As this SFR is mandatory, at least one key generation algorithm shall be included in the scope. |
| REQ | When a trusted subsystem is used for some, or all, of this function, the Chip Vendor shall describe which set of cryptographic operations is performed by the trusted subsystem. |

### Cryptographic KeyStore

The platform provides a way to store <list of assets, such as cryptographic keys and passwords> such that not even the application can compromise the <selection: authenticity, integrity, confidentiality> of this data. This data can be used for the cryptographic operations <list of operations>.

|  |  |
| --- | --- |
| REQ | This SFR addresses all the cryptographic key storage functionality available to the NSPE. As this SFR is mandatory, at least one cryptographic algorithm shall be included in the scope. |
| REQ | The cryptographic keys used internally by the platform shall be also described in this SFR, including the HUK, ROTPK, IAK secure storage key and boot decryption key (if supported).  |
| *REQ*  | PSA requires minimum security strength in line with the current version of NIST SP800-57 pt 1 recommendations. |
| *INFO*  | RSA-2048 will be accepted in products certified before the end of 2026. |
| REQ | When a trusted subsystem is used for some, or all, of this function, the Chip Vendor shall describe which cryptographic keys are stored on the trusted subsystem. |

## Optional Security Functional Requirements

### Audit Log Generation and Storage

The platform generates and maintains an audit log of <list of significant security events> and allows access and analysis of these logs following a specific <access control policy>.

|  |  |
| --- | --- |
| INFO | The developer can choose whether to implement this functionality and claim the SFR or not to implement it and not claim the SFR. |

### Software Attacker Resistance: Isolation of Application Parts (between each of the Application Root of Trust services)

The platform provides isolation between parts of the application, such that an attacker able to run code as one of the **Application Root of Trust Secure Partitions** cannot compromise the **confidentiality and** integrity of the other application parts.

|  |  |
| --- | --- |
| INFO | Additional isolation boundaries between each of the Application RoT services. |

### Secure Debugging

The platform only provides <list of endpoints> authenticated as specified in <specification> with debug functionality.

The platform ensures that all user data stored, with the exception of <list of exceptions>, is made unavailable.

|  |  |
| --- | --- |
| REQ | If the platform implements secure debugging, this SFR shall be included in the ST as it addresses the authenticated access to the PSA-RoT debug functionality. However, in case that debug features are deactivated prior to the final product is delivered to the end-user, this SFR can be removed. |

### Secure Encrypted Storage

The platform ensures that all user data stored, except for <list of data stored in plaintext>, is encrypted as specified in <specification> with a platform instance unique key of key length <key length>.

|  |  |
| --- | --- |
| REQ | For the secure storage functionality, the developer shall claim in its product security target at least one of the following SFRs:* Secure Encrypted Storage
* Secure Confidential Storage
 |
| REQ | Secure encrypted storage requires confidentiality and integrity. |
| REQ | Data stored shall be bound to the unique instance of the platform. |
| INFO | This SFR can be claimed for the implementation of the Internal Trusted Storage API [PSA-SS] when the confidentiality and integrity properties rely on cryptographic means.  |
| REQ | The scope is all data stored in any memory included in the scope of the evaluation.When a trusted subsystem is used for some, or all, of this function, the Chip Vendor shall describe which set of assets is managed by the trusted subsystem. In cases where data is also stored in a memory which is out of the scope of the evaluation, the “Secure Data Serialization” SFR shall be also claimed.  |

### Secure Confidential Storage

The platform ensures that all data stored, except for <list of data stored>, is protected to ensure its confidentiality, integrity, authenticity, and binding to the platform instance.

|  |  |
| --- | --- |
| *REQ* | For the secure storage functionality, the developer shall claim in its product security target at least one of the following SFRs:* Secure Encrypted Storage
* Secure Confidential Storage
 |
| *INFO* | This SFR can be claimed for the implementation of the Internal Trusted Storage API [PSA-SS] when the confidentiality, integrity and authenticity properties rely on access control mechanisms.  |
| *INFO* | The scope is all data stored in any memory included in the scope of the evaluation. In cases where data is also stored in a memory which is out of the scope of the evaluation, the “Secure Data Serialization” SFR shall be also claimed.  |

### Secure Trusted Storage

The platform ensures that all user data, except for <list of data stored in plaintext>, is protected to ensure its integrity, authenticity, and binding to the platform instance.

|  |  |
| --- | --- |
| INFO | This SFR can be claimed for the implementation of the Internal Trusted Storage API [PSA-SS] when the integrity and authenticity properties rely on cryptographic means.  |
| INFO | The scope is all data stored in any memory included in the scope of the evaluation. In cases where data is also stored in a memory which is out of the scope of the evaluation, the “Secure Data Serialization” SFR shall be also claimed.  |

### Secure Data Serialization

The platform ensures that all data stored outside the direct control of the platform, except for <list of data stored outside the direct control of the platform>, is protected such that the **authenticity, integrity, confidentiality** <and binding to the platform instance, versioning> is ensured.

|  |  |
| --- | --- |
| REQ | This SFR shall be claimed if the platform data is stored in a memory out of the scope of the evaluation, such as a removable or on-PCB Flash, or a cloud-storage service. |
| *INFO* | This SFR can be claimed for the implementation of the Protected Storage API [PSA-SS].  |
| INFO | Protection of the cryptographic material used for secure serialized data will rely on one of the mandatory Secure Encrypted Storage or Secure Confidential Storage SFR. |

### Limited Physical Attacker Resistance

The platform detects or prevents attacks by an attacker with physical access before the attacker compromises Verification of Platform Identity, Secure Update of Platform, Secure Initialization and <list of Security Functional Requirements>.

|  |  |
| --- | --- |
| INFO | A Trusted Subsystem used in the implementation of a PSA-RoT is an example of a PSA certifiable RoT Component.  |
| INFO | A Trusted Subsystem may comprise both hardware and software elements. |
| REQ | This SFR is mandatory for all certification to Level 2+SE. |
| REQ | The developer shall describe the mechanism that is used to protect in confidentiality and integrity the communication between the Trusted Subsystem and the Host Platform. |
| REQ | Level 2+SE requires the link to be protected to prevent attacks such as probing to reveal secrets. Typically, this means use of cryptography where the link is easily accessible, for example, on a PCB trace or a physical pin of a device. An on-chip Trusted Subsystem shall be shown to be accessible only by the SPE, this may be achieved by use of cryptography or by physical means. |
| REQ | The list of SFRs protected shall include all functions performed on the Trusted Subsystem |

### Secure Communication Support

The platform provides one or more secure communication channel(s).

The secure communication channel authenticates <list of endpoints> and protects against <list of attacks including disclosure, modification, replay, erasure> of messages between the endpoints, using <list of protocols and measures>.

|  |  |
| --- | --- |
| INFO | If the platform provides multiple different secure channels, this SFR should be iterated for each channel type. |

### Secure Communication Enforcement

The platform ensures that communication with <list of endpoints> can only be done over the secure communication channel(s) supported by the platform using <list of protocols and measures>.

|  |  |
| --- | --- |
| INFO | The ST must include an iteration of Secure Communication Support for each secure channel type referenced in this SFR. |

# Mapping and Sufficiency Rationales

## Assurance

The assurance activities defined in [PSA-EM-L2] fulfil the SESIP2 activities. In particular, the required source code review, vulnerability analysis and testing to an equivalent of 25 person-days of the [PSA-EM-L2] is applicable.

|  |  |
| --- | --- |
| REQ | This section shall be completed by the ST writer. |

| Assurance Class | Assurance Family | Covered by |
| --- | --- | --- |
| ASE: Security Target evaluation | ASE\_INT.1 ST Introduction | <Section “Introduction” and title page of the Security Target> |
| Rationale: |
| ASE\_OBJ.1 Security requirements for the operational environment | <Section “Security Objectives for the Operational Environment” of the Security Target> |
| Rationale: |
| ASE\_REQ.3 Listed Security requirements | <Section “Security Requirements and Implementation” of the Security Target> |
| Rationale: |
| ASE\_TSS.1 TOE Summary Specification | <Section “Security Requirements and Implementation” of the Security Target> |
| Rationale: |
| ADV: Development | ADV\_FSP.4 Complete functional specification | <Description of which developer evidence is used to meet this requirement> |
| Rationale: |
| AGD: Guidance documents | AGD\_OPE.1 Operational user guidance | <Description of which developer evidence is used to meet this requirement> |
| Rationale: |
| AGD\_PRE.1 Preparative procedures | <Description of which developer evidence is used to meet this requirement> |
| Rationale: |
| ALC: Life-cycle support | ALC\_FLR.2 Flaw reporting procedures | <ALC\_FLR section in the Security Target and description of which developer evidence is used to meet this requirement> |
| Rationale: |
| ATE: Tests | ATE\_IND.1 Independent testing: conformance | <Description of which developer evidence is used to meet this requirement> |
| Rationale: |
| AVA: Vulnerability Assessment | AVA\_VAN.3 Focused vulnerability analysis | Vulnerability and testing carried out by the laboratory |
| Rationale: |

Table 7: Assurance Mapping and Sufficiency Rationales

# Appendix: SFRs by PSA Certified Levels

The following table summarizes the required SFRs according to PSA Certified Levels. In this table, Y stands for mandatory SFR, O for optional SFR and N/A for not applicable for this level.

|  |  |  |  |
| --- | --- | --- | --- |
| PSA Certified Level | Level 2 |  Level 3 | Level 3 iSE/SE or Level 4 iSE/SE |
| **Scope** | PSA-RoT | PSA-RoT | Trusted Subsystem |
| **Evaluation Methodology** | SESIP Level 2 | SESIP Level 3 | SESIP Level 3 |
| **Attack Resistance** | 0-15 | 0-20 | 0-20 (Level 3)0-24 (Level 4) |
| **Mandatory SFRs** |  |
| Verification of Platform Identity | Y | Y | Y |
| Verification of Platform Instance Identity | Y | Y | O |
| Attestation of Platform Genuineness | Y | Y | O |
| Secure Initialization of Platform | Y | Y | Y |
| Attestation of Platform State | Y | Y | O |
| Secure Update of Platform  | Y | Y | Y |
| Physical Attacker Resistance | N/A | Y | Y |
| Software Attacker Resistance: Isolation between SPE and NSPE | Y | Y | Y |
| Software Attacker Resistance: Isolation between PSA-RoT and Application RoT | Y | Y | Y |
| Cryptographic Operation | Y | Y | Y |
| Cryptographic Random Number Generator | Y | Y | Y |
| Cryptographic Key Generation | Y | Y | Y |
| Cryptographic KeyStore | Y | Y | Y |
| Secure Storage (At least one of Secure Encrypted Storage, Secure Confidential Storage or Secure Trusted Storage) | Y | Y | O |
|  |
| **Additional SFRs** |  |
| Secure Communication Support | N/A | N/A | (1) |
|  |
| **Optional SFRs** |  |
| Audit Log Generation and Storage | O | O | O |
| Software Attacker Resistance: Isolation of Application Parts (between each of the ARoTs) | O | O |  |
| Secure Debugging | O | O | O |
| Limited Physical Attacker Resistance | O | N/A | N/A |
| Secure Data Serialization | O | O |  |
| Secure Communication Support | O | O |  |
| Secure Communication Enforcement | O | O |  |

Table 8 SFRs by PSA Certified Levels

For iSE/SE, the Secure Communication Support SFR marked with (1) must be included into the security target if protection of the link between the Host Platform and the iSE/SE relies on cryptographic means (as opposed to access control means).